**Question 1**

The segment registers have assigned for different task from storing variable data. Basically it stores stack address. To reference any memory location in a segment, the processor combines the segment address in the segment register with the offset value of the location. So that, it’s not a ideal idea to store data inside of Segment register.

**Question 2**

General purpose of registers -

* AX : To store input data
* BX : Store offset value
* CX : counter data for control statement
* DX : Data register to execute operation